**NUC-G BIOS ENGINEERING**

****

Intel Corporation, 5200 NE Elam Young Parkway  
Hillsboro, OR 97124-6497

BIOS Update Release Notes

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0070.2022.1103.1527 Production BIOS

**About This Release:**

* Date: 11/03/2022
* ROM Image Checksum: 0xCCB5D121
* EC Firmware: 0E.0B.00 (11.00)
* **ME Firmware: 11.8.93.4323 (v3)**
* CRB Label: 1ATQO051
* Boot Guard ACM: 3698
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_19
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:
  + WinBond W25Q128JVSIQ 16MB
  + MACRONIX MX25L12850F 16MB
  + GigaDevice GD25B127D 16MB
* Microcode Updates included in .BIO & .ROM Files:
  + **M2A906E9\_000000EF\_000000F0**

**New Fixes/Features/Updates:**

Based on HN0069

* Fixed: [AMI Changes][EIP 711621][PTK2696] Intel NUC information disclosure vulnerability.
* Fixed: [AMI Changes][EIP 711511][PTK2619] BIOS stack buffer overflow vulnerability.
* Fixed: [AMI Changes][EIP701358[ [PTK1729] Unauthorized modification of UEFI variables.
* Fixed: [AMI Changes][EIP 709238][PTK2712/SA50151] SIO\_DEV\_STATUS\_VAR\_NAME Information Leakage\_PTK2712#12.
* Fixed: [AMI Changes][EIP 709047][PTK2911/SA50133] RSB Stuffing Mitigation for Speculative Execution Vulnerability.
* Fixed: [AMI Changes][EIP 709152][SA50085/PTK2912] GRUB Bootloader Vulnerability.
* Fixed: [AMI Changes][EIP 709150][SA50088] TianoCore Security Issues.
* Fixed: [AMI Changes][EIP 709048][PTK2828/PTK2829] Intel NUC 8 vulnerability/Intel NUC 8 info leak vulnerability.
* Added: [AMI Changes][EIP 709039][SA50120] BootPerformanceTable\_pointer.
* Updated: [AMI Changes][EIP 709237] 2022 IPU update: 2022.1/2022.3.
* Fixed:[AMI Changes][EIP 711704] POST hang at Intel NUC logo splash screen with Windows 10 20H1.
* **Updated: [BIOS0069] ME FW to CSME\_11.8.93.4323v3\_Consumer.**
* **Updated: [BIOS0069] CPU Microcode to M2A906E9\_000000EF\_000000F0.**

**Known Errata:**

* Config Menu:[2] Clear BIOS User and Supervisor Passwords function doesn't work; the passwords can't be cleared.
* Boot Menu doesn't show the bootable NVMe SSD installed on the Thunderbolt enclosure adapter.(Boot Menu can show the bootable USB drive installed on the Thunderbolt dock.)
* **Blocked BIOS F7 Flash downgrade to HN0067 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

### HNKBLi70.86A.0069.2022.0923.1821 Development BIOS

**About This Release:**

* Date: 09/23/2022
* ROM Image Checksum: 8f88
* EC Firmware: 0E.0B.00
* **ME Firmware: 11.8.93.4323**
* CRB Label: 1ATQO051
* Boot Guard ACM: 3698
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + UEFI Driver: 9.0.1074
* Intel RST Pre-OS:
  + VMD UEFI Driver: NA
* AHCI Code: AHCI\_19
* Supported Flash Devices:
  + WinBond W25Q128JVSIQ 16MB
  + MACRONIX MX25L12850F 16MB
  + GigaDevice GD25B127D 16MB
* Microcode Updates included in .BIN & .CAP Files:
  + **m2a906e9\_000000ef\_000000f0**

**Security Patch:**

* eip701357 [PTK1885] Unauthorized modification of UEFI variables
* eip701358 [PTK1729] Unauthorized modification of UEFI variables
* eip701359 [PTK1893] Unauthorized modification of UEFI variables
* eip701361 [PTK1947] Unauthorized modification of UEFI variables
* eip701364 [PTK2622] Unauthorized modification of UEFI variables
* eip702508 [PTK1931] Privilege escalation vulnerability from kernel to SMM in multiple devices
* eip703170 [PTK2867/SA50131] S3 Resume Unprotected Ptr

**Feature Change/Update:**

* **Updated ME FW CSME\_11.8.93.4323v3\_Consumer**
* **Updated CPU Microcode m2a906e9\_000000ef\_000000f0**

**Known Errata:**

* Block F7/EBU downgrade to HN0067 due to ME update.

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0067.2021.0528.1339 Production BIOS

**About This Release:**

* Date: May 28, 2021
* ROM Image Checksum: 0x44E6, 0xA37F (NOBG)
* **ME Firmware: 11.8.86.3909**
* EC Firmware: 0E.0B.00 (11.00)
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

**M2A906E9\_000000EA.pdb**

**New Fixes/Features:**

* Based on HN0066
* **Updated: ME FW version to 11.8.86.3909**
* EIP572366 [SPG-HN][Pega]Fixed: 22011533606 Seagate FireCuda 520 SSD boot issues with HN0063.
* EIP605733 [Intel-SPG][PEGA][HN] Updated OFBD module SMI handler vulnerabilities.
* EIP611164 [Intel-SPG][PEGA][HN] Added protection code for unauthorized write at controllable address in SMRAM.
* EIP613600 [Intel-SPG][PEGA][HN] Added: ACPI improvement for "PTK1456 Memory corruption during S3 resume".
* **EIP613609 [Intel-SPG][PEGA][HN] Updated: CPU Microcode for IPU 2021.1:**
* **M2A906E9\_000000EA.pdb**
* EIP614689 [Intel-SPG][PEGA][HN][PTK1484] Fixed: Able to achieve arbitrary write in SMRAM save state region.

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0066 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0066.2021.0310.1823 Production BIOS**

**About This Release:**

* Date: Mar 10, 2021
* ROM Image Checksum: 0xB46E, 0x1307 (NOBG)
* ME Firmware: 11.8.83.3874
* EC Firmware: 0E.0B.00 (11.00)
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000DE.pdb

**New Fixes/Features:**

* Based on HN0064
* Update: ME FW version to 11.8.83.3874.
* Update: Updated NTFS\_06 for "Heap corruption and denial of service in NTFS DXE driver in process of parsing NTFS file system partition".
* Updated: EC FW to 0E.0B.00 (11.00)
* Fixed: Customers reporting that Hades LEDs (front and skull) no longer work in S0 after updating to BIOS 0064.

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0065 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0065.2021.0113.1340 Production BIOS**

**About This Release:**

* Date: Jan 13, 2021
* ROM Image Checksum: 0x3BBA, 0x9A53 (NOBG)
* ME Firmware: 11.8.82.3838
* EC Firmware: 0E.0A.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000DE.pdb

**New Fixes/Features:**

* Based on HN0064
* Update ME FW version to 11.8.82.3838

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0064 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0064.2020.1028.1438 Production BIOS**

**About This Release:**

* Date: Oct 28, 2020
* ROM Image Checksum: 0x6D44, 0xCBDD (NOBG)
* ME Firmware: 11.8.80.3746
* EC Firmware: 0E.0A.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM:
  + - i219: 7.5.11
    - i211: 0.0.17
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000DE.pdb

**New Fixes/Features:**

* Based on HN0063
* Updated: ME firmware to 11.8.80.3746, Microcode firmware to 0xDE.
* Fixed: “Front USB 3.0 port could not be used”.
* Fixed: “Previously programmed NVMe M.2 SSD Admin password shows as "NOT INSTALLED" in Visual BIOS”.
* Fixed: “Analog audio output sample rate support”.
* Fixed: “SATA M.2 SSD type not displayed in SATA section under Visual BIOS DEVICE”.
* Fixed: “Hades Canyon USB port power issue”.
* Fixed issue where “Arbitrary code execution at PEI phase (WakeUpType)”.
* Fixed issue where “SMRAM overwritten with arbitrary data (microcodeUpdate).

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0062 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0063.2020.0827.1309 Production BIOS**

**About This Release:**

* Date: Aug 27, 2020
* ROM Image Checksum: 0x6AE8, 0x4CFD (NOBG)
* ME Firmware: 11.8.79.3722
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000D6.mcb

**New Fixes/Features:**

* Based on HN0062
* Updated ME FW version to 11.8.79.3722.
* Fixed issue where “Native ACPI OS PCIe Support can’t be enabled in BIOS if Thunderbolt Controller is enabled”.
* Fixed issue where “System BSoD during restart Windows 10 20H1 (2004)(SGX Driver v2.7.101.2)”.

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0062 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0062.2020.0813.2317 Production BIOS**

**About This Release:**

* Date: Aug 13, 2020
* ROM Image Checksum: 0x5A64, 0x3C79 (NOBG)
* ME Firmware: 11.8.70.3626
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000D6.mcb

**New Fixes/Features:**

* Based on HN0061
* Updated: NVME module to Label 26.
* Updated: TcgStorageSecurity driver.
* Fixed issue where systems with BIOS HN0060 & 0061 cannot boot with certain models of SSD installed:
  + ADATA XPG SSD
  + WD Blue SN550
  + Crucial MX500/P1
  + Intel 600p/660p/760p
  + HP EX900

**Known Errata:**

* **Downgrading to BIOS 0059 is only possible by using Jumper Recovery method.**
* **Blocked BIOS F7 Flash/EBU downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

**HNKBLi70.86A.0061.2020.0617.1539 Production BIOS**

**About This Release:**

* Date: June 17, 2020
* ROM Image Checksum: 0xFB69, 0xDD7E (NOBG)
* ME Firmware: 11.8.70.3626
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000D6.mcb

**New Fixes/Features:**

* Based on HN0060
* Fixed [Intel-SPG][PEGA][HN] Microcode update for PSIRT.
* Fixed [SPG-HN][PEGA][Security] SA00289 PSIRT update.
* Fixed issue where “[Intel-SPG][PEGA][HN] Arbitrary code execution in SMM due to insufficient buffer validation.”
* Improved BIOS code:

>> Fixed [Intel-SPG][PEGA][HN] Lock Manufacturing mode abnormal behavior.

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0060.2020.0318.1619 Production BIOS

**About This Release:**

* Date: March 18, 2020
* ROM Image Checksum: 0xABDD, 0x8DF2 (NoBG)
* ME Firmware: 11.8.70.3626
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000B4.mcb

**New Fixes/Features:**

* Based on HN0059
* Fixed PSIRT issues:

>> Updated ME to 11.8.70.3626.

>> Fixed issue where “Intel NUCs bypassing EFI variables protection (microcode downgrade still possible)”.

>> Fixed issue where “AHCI int13 smi driver vulnerable for OOB read”.

* Fixed issue [HSD-ES][client\_platf][bug][2209242185][]ICS - HN - BIOS53-58 Security bug: Not able to read SSD Admin Passwords created using BIOS 0052.
* Fixed issue [HSD-ES][client\_platf][bug][2209673523][]ICS: NUC8i7HNK, Deep S4/S5 setting not saved in BIOS.
* Fixed issue ICS - HN - BIOS53-58 Security bug: Not able to create Admin Passwords on SSDs.
* Fixed issue [HSD-ES][client\_platf][bug][2209242354][]ICS - HN - BIOS Feature Enhancement: Not able to Set Admin Password on both (2) installed SSDs.
* Fixed issue where “Set default Family Name” for Microsoft request.
* Fixed issue where “Energy star logo show on Tencent SKU(NUC8i7HVKVAW)”.
* Fixed issue where ICS: DN - PXE boot - “Press F12 for network service boot” message not displayed in UEFI.

**Known Errata:**

* **Blocked BIOS F7 Flash/EBU downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0059.2019.1112.1124 Production BIOS

**About This Release:**

* Date: Nov 12, 2019
* ROM Image Checksum: 0x03BE, 0xE770(NoBG)
* ME Firmware: 11.8.60.3561
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000B4.mcb

**New Fixes/Features:**

* Based on HN0058
* Improved BIOS code.

>> Fixed issue where “WHQL USB3 Termination test fail”

>> Fixed Hybrid BIOS USB recovery

>> Fixed Intel NUC and Energy Star Logo

* Fixed PISRT issue.

>> Fixed issue where “CVE-2019-11094 Insufficient mitigation”

>> Fixed issue where “Attacker with a sufficient level of privileges can inject malicious code into the firmware”

>> Fixed issue where “PCR reset vulnerability of Intel Platform Trusted Technology (firmware TPM)"

>> Fixed issue where “Intel NUCs SMM code execution during the boot phase"

* Fixed: SMBIOS Field update BIOS for Microsoft request.
* Fixed: Chassis value type changed flash by BIO for Microsoft request.

**Known Errata:**

* **Blocked BIOS flash downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0058.2019.0705.1646 Production BIOS

**About This Release:**

* Date: July 05, 2019
* ROM Image Checksum: 0x9377, 0x7729(NoBG)
* ME Firmware: 11.8.60.3561
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000B4.mcb

**New Fixes/Features:**

* Based on HN0057
* Fixed issue where [HSD-ES][client\_platf][bug][2206851920][]ICS: Hades: TPM disappears from Windows after power loss
* Fixed issue where “WHQL USB Exposed Port System Test” fails.
* Fixed issue where [HSD-ES][client\_platf][bug][platform.NUC.Hades Canyon][2207747905][p3-medium][open] ICS: HN - The power button never turns orange when using the Power Button Recovery process.
* Modified BIOS code for security fixes.

>> Fixed issue where “FW-UEFI-Vuln-2019-006 NUC SMRAM arbitrary write through the SMI handler's stack usage and SW SMI call-out”

>> Fixed issue where “Integer overflow SMM-module AhciInt13Smm on Intel NUC Kit”

**Known Errata:**

* **Blocked BIOS flash downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0057.2019.0528.1518 Production BIOS

**About This Release:**

* Date: May 28, 2019
* ROM Image Checksum: 0xDBAD, 0xBF5F(NoBG)
* ME Firmware: 11.8.60.3561
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_000000B4.mcb

**New Fixes/Features:**

* Based on HN0056
* Modified BIOS code for security fixes.

>> Fixed NUC SW SMI call-out NVMe.

>> Fixed BIOS lack of update authentication.

>> Updated ME FW to 11.8.60.3561-SA00185 security advisory- ME update.

>> Updated Microcode to M2A906E9\_000000B4 Microarchitecture Data Sampling for PSIRT-TA-2019-02-002.

**Known Errata:**

* **Blocked BIOS flash downgrade to HN0056 and previous versions due to ME FW update.**
* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0056.2019.0506.1527 Production BIOS

**About This Release:**

* Date: May 06, 2019
* ROM Image Checksum: 0xFB058, 0xE243(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_0000008D\_0000008E.PDB

**New Fixes/Features:**

* Based on HN0055
* BIOS improvement.

>>Added workaround to display Energy Star LOGO for 2 seconds.

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

### HNKBLi70.86A.0055.2019.0424.1629 Production BIOS

**About This Release:**

* Date: Apr 24, 2019
* ROM Image Checksum: 0xF0B5, 0xD7A0(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO Files:

M2A906E9\_0000008D\_0000008E.PDB

**New Fixes/Features:**

* Based on HN0054
* Fixed no Energy Star LOGO from HN0050.
* Changed enclosure type default to 0x23.

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0054.2019.0214.1350 Production BIOS

**About This Release:**

* Date: Feb 14, 2019
* ROM Image Checksum: 0x7521, 0x5C0C(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM & .BIO files:

M2A906E9\_0000008D\_0000008E.PDB

**New Fixes/Features:**

* Based on HN0053
* Updated BIOS code for security fixes.

>> Update CryptoPkg module to label CryptoPkg\_32.01 for OpenSSL.

>> Fixed OverClockSMI handler allows read/write of SMRAM.

>> Update module to AmiCpuModulePkg\_027 to prevent CPU Microcode downgrade attack.

>> Removed additional DMAR RMRR table for external USB.

>> Update module to HddSecurity\_24

>> Fixed TcGSmm driver contain code that potentially exposes a smram attack.

>> Fixed FlashSmiSmm driver vulnerable to SMRAM memory write attack.

>> Fixed SmmPcieSataController driver vulnerable to SMRAM memory write attack.

>> Fixed Insufficient validation done on a user-controlled data structures while executing particular SMI handlers leads to SMRAM memory corruption

>> Fixed ITKSmmVars potential SMM privilege escalation.

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0053.2018.1217.1739 Production BIOS

**About This Release:**

* Date: December 17, 2018
* ROM Image Checksum: f88e,df79(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed issue where [HSD-ES] [client\_platf] [bug] [2205368114] ICS: HN/KY/BN - Samsung eDrive stopped working.
* BIOS code improvement.

>>Updated TCG2 module to TCG2\_18

>>Updated NVME module to NVME\_19

>>Update TcgStorageSecurity module to TcgStorageSecurity\_04

>> Fixed OPAL password pop up when Windows 10 BitLocker is enabled.

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0052.2018.1129.1700 Production BIOS

**About This Release:**

* Date: November 29, 2018
* ROM Image Checksum: d9b2,c09d(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0

Integrated Graphics:

* + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* BIOS code improvement.

>> Changed ITK boot count for manufacturing line to 25.

>> Modified code to speed up boot time to Intel NUC logo.

>> Fixed ME loss when “After Power Failure” set to power on.

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0051.2018.1024.1600 Production BIOS

**About This Release:**

* Date: October 24, 2018
* ROM Image Checksum: d4e1,c7f6(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Based on HN0050.
* Fixed issue where [HSD-ES][client\_platf][bug][2205484449][]ICS: HNK - Error when trying to install ESXi 6.5 or 6.7
* Fixed issue where [HSD-ES][client\_platf][bug][2205447768][]ICS: HN - HNK won't install some Linux Distros with Secure Boot
* Fixed issue where [HSD-ES][client\_platf][bug][2205434578][]ICS: HN - Windows not showing Memory Speed Correctly

**Known Errata:**

* **ITK 5 based EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0050.2018.0927.1020 Production BIOS

**About This Release:**

* Date: September 27, 2018
* ROM Image Checksum: 957d, 8892(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - * Option ROM: 9.0.1051
      * UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Based on HN0049
* BIOS code improvement.

>> Fixed issue where LAN boot will be set as the 1st priority Boot device when 1st boot up.

>> Fixed issue where cannot receive CEC QEvent from EC.

>> Fixed issue where when Fast Boot is enabled and RAID changed to AHCI mode, system hangs at POST.

* Fixed issue where HSD 1407352212ICS: HN - SMBIOS Table Structure Issues.
* Fixed issue where HSD 1407352212 HN-Fast Boot and RAID mode coexistence problem - Visual BIOS.

**Known Errata:**

* **EBU files for INTERNAL Intel use only.**
* **WU files for Intel test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0049.2018.0801.1601 Production BIOS

**About This Release:**

* Date: August 01, 2018
* ROM Image Checksum: e894,dba9(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Added Deep S4/S5 item in BIOS setup.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0048.2018.0725.1749 Production BIOS

**About This Release:**

* Date: July 25, 2018
* ROM Image Checksum: 8c5b,7f70(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Removed Intel Ready Mode code/items in BIOS for Intel security fix.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0047.2018.0718.1706 Production BIOS

**About This Release:**

* Date: July 18, 2018
* ROM Image Checksum: 9879, 8b8e(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed issue where UnCore voltage default was set to 0mV.
* Updated Microcode for Intel SA00115 PSIRT fixes.
* Removed Energy Star logo from showing in China SKU.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0046.2018.0712.1631 Production BIOS

**About This Release:**

* Date: July 12, 2018
* ROM Image Checksum: 4ebc,41d1(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.09.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed issue where [HSD-ES] [client\_platf] [bug] [2203959776] ICS: HN - Updating the BIOS does not work when running some memory modules above 2400MHz.
* Fixed issue where [HSD-ES] [client\_platf] [bug][2204142145] ICS: HN - Does not power on correctly when the power cord is pulled and the BIOS option "After Power Failure" is set to either, "Last State" or "Power On".
* Updated EC FW to 0E.09.00.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

### HNKBLi70.86A.0045.2018.0628.2116 Production BIOS

**About This Release:**

* Date: June 28, 2018
* ROM Image Checksum: d10f,c424 (NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000008D\_0000008E.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Added Windows F8 recovery function
* Updated to the latest microcode.
* Fixed fault tolerance sometimes are not working with BootGuard enabled board
* Added negative value for Core and Uncore voltage.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0044.2018.0615.1726 Production BIOS

**About This Release:**

* Date: June 13, 2018
* ROM Image Checksum: 1cb4, 0fc9(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Changed verb table for DMIC function.
* Refine Energy-Star LOGO provided by Intel team.

**Known Errata:**

* **EBU files are for INTERNAL Intel use only.**
* **WU files are for test use only.**

### HNKBLi70.86A.0043.2018.0608.1115 Development BIOS

**About This Release:**

* Date: June 07, 2018
* ROM Image Checksum: e6bc,d9d1 (NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed: CIR disable function does not work correctly.
* Fixed: ME FW update not working.
* Changed CIR Enabled in manufacturing mode, Disabled by default.

**Known Errata:**

* None.

### HNKBLi70.86A.0042.2018.0531.0911 Development BIOS

**About This Release:**

* Date: May 31, 2018
* ROM Image Checksum: 5bf7,4d0c(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Added Energy Star Logo on POST if system info product name belongs to an L10 system.
* Updated "ICBDCapsule" module to fix that unsigned BIO file can be used for FW update.

**Known Errata:**

* None.

### HNKBLi70.86A.0041.2018.0524.1105 Development BIOS

**About This Release:**

* Date: May 24, 2018
* ROM Image Checksum: 6273,5388(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.2.0
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 16.0.2.3402
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Updated to CRB 51.
* Updated SATA RAID Option ROM FW to 16.0.2.3402.

**Known Errata:**

None.

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0040.2018.0516.1521 Production BIOS

**About This Release:**

* Date: May 16, 2018
* ROM Image Checksum: D4EF,C604(NOBG)
* ME Firmware: 11.8.50.3460
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed: Plextor SSD hanging issue.
* Updated ME FW to 11.8.50.3460
* Fixed Power button/Skull/Eye LED will present breathing.
* Fixed Power button/Skull/Eye LED default S0 behavior frequency is 0.

**Known Errata:**

* None.

### HNKBLi70.86A.0039.2018.0509.1758 Development BIOS

**About This Release:**

* Date: May 09, 2018
* ROM Image Checksum: 2da9, 1f76(NOBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Fixed: Windows 10 Recovery can enter BIOS setup with User Access level set to No Access.
* Fixed VTinfo test no external USB RMRR entry
* Changed that EC will save to flash with each time LED setup item changes.
* Changed LED behavior default blinking frequency to 10 (1Hz)

**Known Errata:**

* None.

### HNKBLi70.86A.0038.2018.0503.0923 Development BIOS

**About This Release:**

* Date: April 26, 2018
* ROM Image Checksum: 1c72,0e3f(NOBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.08.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Fixed: Issue with Power button, Skull, Eye LED set to any color in Visual BIOS, then reboot to OS, the behavior in S0 cannot recover to default.
* Fixed: Issue with Front LED3 set to single color in OS APP then reboot set to any color in Visual BIOS, it will not recovery to green to red.
* Fixed: Issue with after load defaults in Visual BIOS, LED setting cannot revert back to default under OS
* Fixed: Issue Via "Software LED Control Enabled" to change setting to Software Controlled, LED indicator and behavior cannot back to default.
* Fixed: Issue If only enable Ethernet2 or Both enable Ethernet 1&2, SUT will always boot to LAN boot as first boot device.
* Added USBrt security update.
* Changed verb table from Realtek for beep command.
* Updated EC FW to 0E.08.00

**Known Errata:**

* None.

**Kaby Lake-G Standard BIOS**

**PRODUCTS**: NUC8i7HNK, NUC8i7HVK (Hades Canyon)

### HNKBLi70.86A.0037.2018.0423.0910 Production BIOS

**About This Release:**

* Date: April 23, 2018
* ROM Image Checksum: 0469,F636(NoBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Added Fix: System sometimes cannot shutdown successfully.

**Known Errata:**

* None.

### HNKBLi70.86A.0036.2018.0418.1719 Release Candidate BIOS

**About This Release:**

* Date: April 18, 2018
* ROM Image Checksum:4D35, 3F02 (NoBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed issue that LED don’t load default value for S3 blinking behavior.
* Fixed issue that LED not set S3 color as the color set in BIOS setup.
* Disable and hide the Legacy Boot option in Visual BIOS.

**Known Errata:**

* None.

### HNKBLi70.86A.0035.2018.0412.1113 Development BIOS

**About This Release:**

* Date: April 12, 2018
* ROM Image Checksum: 5acc, 4c99(NoBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed LED Ethernet Indicator Type will change to LAN1 when system enters S3, S4, and S5.
* Fixed M.2 RST remapping in setup menu
* Fixed TBT security level not saved in BIOS setup
* Fixed power button LED will reset to default after reboot.

**Known Errata:**

* None.

### HNKBLi70.86A.0034.2018.0329.1113 Production BIOS

**About This Release:**

* Date: March 29, 2018
* ROM Image Checksum: 32A2,246F(NoBG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Fixed LED WMI not report disabled status correctly
* Added LED blinking in flash update.

**Known Errata:**

* None.

### HNKBLi70.86A.0033.2018.0326.1602 Development BIOS

**About This Release:**

* Date: March 26, 2018
* ROM Image Checksum: 14b2,9951(No BG)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Fixed when F7 flash BIOS from HN0022, NVME device cannot remap to RST
* Set LED to default SW control setting when LED setup item changed from disable to SW control
* Added HDMI hot plug feature for headless operation.

**Known Errata:**

* None.

### HNKBLi70.86A.0032.2018.0314.1912 Development BIOS

**About This Release:**

* Date: March 14, 2018
* ROM Image Checksum: d204
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Reset LED setting after flash BIOS from old version to fix SW control color not correct issue
* Fixed Samsung NVME SSD 950 not show device name in setup menu.

**Known Errata:**

* None.

### HNKBLi70.86A.0031.2018.0308.1050 Development BIOS

**About This Release:**

* Date: March 08, 2018
* ROM Image Checksum: ec7a
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.07.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Added IO Header - Control Power LED porting
* Disabled Post Manufacturing NVAR Configuration
* Fixed F9 load default not load LED options default
* Fixed Secondary LAN will be disable when disable Primary LAN
* Fixed fastboot enable will present win logo
* Hide LED Reset item from Visual BIOS
* Updated EC FW to 0E.07.00

**Known Errata:**

* None.

### HNKBLi70.86A.0030.2018.0301.1049 Development BIOS

**About This Release:**

* Date: March 01, 2018
* ROM Image Checksum: b7f3, 6897(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.06.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Fixed FP1~FP3 no default S3 behavior
* Fixed LED disable indicator behavior
* Fixed NewGetLedStatus cannot get indicator
* Fixed SW control indicator cannot set and get correctly
* Fixed SW control indicator color cannot be set
* Fixed MAC Address information can’t read after disable "Network Boot" in setup
* Changed USB driving ability porting.

**Known Errata:**

* None.

### HNKBLi70.86A.0029.2018.0222.1359 Production BIOS

**About This Release:**

* Date: February 22, 2018
* ROM Image Checksum: CE4B,7EEF(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.06.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_00000083\_00000084.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_00000083\_00000084.PDB

**New Fixes/Features:**

* Updated microcode to 84.
* Updated EC FW to 0E.06.00

**Known Errata:**

* None.

### HNKBLi70.86A.0028.2018.0213.1200 Development BIOS

**About This Release:**

* Date: February 13, 2018
* ROM Image Checksum: 1acb,cb6f(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.05.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added TBT SxExit delay
* Added i210 pxe legacy rom
* Added new EC config for max duty cycle
* Added new fan curve
* Added psys porting
* Change NetworkBoot default value to disabled
* Disabled iSST by default
* Enabled/Disabled LAN1 UEFI PXE Boot by setup item
* Fixed ATI HDA SSID incorrect
* Fixed BEL fail item: 3 attempts with invalid password
* Fixed LED WMI NewGetLedStatus fail
* Fixed LED WMI can change when not set to SW control
* Fixed NVME device not showing Remapped to RST
* Fixed S3/S4/S5 reset LED setting to default
* Hide cec standby TV item temporarily
* Removed Deep S4/S5 setup item
* Updated EC FW to 0E.05.00.

**Known Errata:**

* None.

### HNKBLi70.86A.0027.2018.0205.1423 Development BIOS

**About This Release:**

* Date: February 05, 2018
* ROM Image Checksum: 8613, 36B7(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.04.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added CIR wake S345 porting
* Changed CEC standby by tv S3 porting with Q-event 0xE3
* Changed Fan speed monitor to one CPU FAN
* Changed Psys setting board id check method
* Changed PsysPmax to 230W
* Changed USB2.0 driving ability
* Fixed LAN2 setting cause razor core cannot work
* Fixed fan off temperature maximum value

**Known Errata:**

* None.

### HNKBLi70.86A.0026.2018.0129.1924 Development BIOS

**About This Release:**

* Date: January 29, 2018
* ROM Image Checksum: d2a2,8346(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.03.00
* Memory Reference Code: Based on 3.0.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added CEC S3 0x29 command
* Added EC BoardID\_HW\_State check
* Changed SATA TX porting
* Changed GPIO porting for UCM
* Fixed F10 select SSD showing windows logo
* Fixed set HDD user password then boot to OS will show windows logo
* Fixed fan not showing FAN1,FAN2
* Fixed LED S3 default
* Fixed Samsung NVME SSD not show VDID on pci tab
* Fixed secondary lan mac address not show
* Fixed some performance item still can change with user access view only
* Fixed temperature display
* Removed CRB setup items in AddIn
* Revert microcode to 70
* Updated EC FW to 0E.03.00.

**Known Errata:**

* None.

### HNKBLi70.86A.0025.2018.0122.1928 Development BIOS

**About This Release:**

* Date: January 22, 2018
* ROM Image Checksum: 616D, 1211(FVME)
* ME Firmware: 11.8.50.3434
* EC Firmware: 0E.02.00
* Memory Reference Code: Based on 3.0.1
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1074
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000007F\_00000080.PDB

* Additional Microcode Updates included only in .BIO File:

None

**New Fixes/Features:**

* Added CIR Controler Type setup item
* Added EC flag clear event function
* Added set EC readCPUTempEnable\_H2RAM flag in PEI
* Changed PCIE RP5 ASPM to Disable
* Changed PCIE RP5 L1 Substates to Disable
* Changed TBT Enable ASPM to Disable
* Changed TBT Reserve I/O to 0
* Changed TBT Reserve IO per phy slot to 0
* Changed TBT USB boot and TBT boot default to disable
* Enabled SPI lock
* Fixed CIR controller type behavior
* Fixed TBT security level
* Fixed WHQL Secure Boot Test
* Fixed WHQL USB Exposed Port System Test fail
* Fixed after rebooting from setting up the profile, the memory Reference Multiplier is disappeared.
* Fixed blue screen when connecting PCI-E device thru TBT
* Removed DGPU ROM
* Removed TBT test delay
* Set EC 0x5F8~0x5FB to 0 when setup item HDMI CEC Control set to disable
* Updated EC FW to 0E.02.00
* Updated ME FW to 11.8.50.3434
* Updated fan curve
* Updated microcode.

**Known Errata:**

* None.

### HNKBLi70.86A.0024.2018.0111.1842 Development BIOS

**About This Release:**

* Date: January 10, 2018
* ROM Image Checksum: f5fe,a62c(FVME)
* ME Firmware: 11.8.50.3425v2
* EC Firmware: 0D.05.00
* Memory Reference Code: Based on 2.9.3
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1015
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Changed Internal Graphics to Intel iGD
* Changed PEG1 for Asmedia USB MaxLinkSpeed to auto
* Changed Performance page for XTU interface
* Changed PowerDefault Balanced & Max Performance Packge Power Time Window (Tau) from 70s to 64s
* Changed PowerDefault VR Current Limits (ICC max Amps) Max value for 150 to 125
* Changed SATA RX porting
* Fixed LED SW control gray out LED items
* Fixed LED SW control help string
* Fixed LED all on not on, now LED will return to default setting
* Fixed LED disable not function
* Fixed LED no default S3 behavior
* Fixed SATA device not show in setup SATA tab when set to RAID mode
* Fixed Suppress Alert Messages At Boot default value
* Fixed SUT will hang on when Press Ctrl+I enter to RAID menu.
* Fixed USB port 3,4 not disable USB 3.0 device
* Fixed WLAN cannot disable
* Fixed i2c not enable for UCM device
* Fixed network boot not load default
* Updated EC FW to 0D.05.00

**Known Errata:**

* None.

### HNKBLi70.86A.0023.2018.0105.1903 Development BIOS

**About This Release:**

* Date: January 05, 2018
* ROM Image Checksum: 510f, 013d(FVME)
* ME Firmware: 11.8.50.3425v2
* EC Firmware: 0D.04.00
* Memory Reference Code: Based on 2.9.3
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added LED setup tab new items
* Added back secondary temperature monitor
* Added performance changes
* Changed SATA RX porting
* Changed secondary temperature monitor default and options
* Changed Internal Graphics to Intel iGD
* Fixed Allow UEFI 3rd party driver loaded help string
* Fixed CPU FAN Header help string
* Fixed Num lock not present in setup menu
* Fixed SD Card "read only" option not present
* Fixed SUT will hang on when Press Ctrl+I enter to RAID menu
* Fixed Thunderbolt still can work after disabled "Thunderbolt Controller" on BIOS Setup.
* Fixed Thunderbolt usb device could boot when disable Thunderbolt USB Boot under BIOS setup
* Fixed USB Port 06[Charging Port] no set to gray out and disable when Portable Device Charging Mode set to Charging Only.
* Fixed USB not charging in S345
* Fixed USB port set to "no detect" still can detect in F10 menu
* Fixed default setting of Ignore Thunderbolt Option Rom is disable
* Fixed when connecting SATA SSD to con5601 not show in setup menu
* Fixed when setup HDD/LAN LED color change, indicator change to power indicator
* Fixed must Press F4 continuously to boot to BIOS recovery
* Removed PCI subsystem options from AddIn tab
* Removed first 6 items in PCI tab

**Known Errata:**

* None.

### HNKBLi70.86A.0021.2017.1228.1615 Development BIOS

**About This Release:**

* Date: December 28, 2017
* ROM Image Checksum: 0de0
* ME Firmware: 11.8.50.3425v2
* EC Firmware: 0D.04.00
* Memory Reference Code: Based on 2.9.3
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed MFGDMI2 tool manufacturing mode not set.

**Known Errata:**

* None.

### HNKBLi70.86A.0020.2017.1227.1625 Development BIOS

**About This Release:**

* Date: December 27, 2017
* ROM Image Checksum: B05D
* ME Firmware: 11.8.50.3425v2
* EC Firmware: 0D.04.00
* Memory Reference Code: Based on 2.9.3
* Integrated Graphics:
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1015
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added PCIE RX driving porting
* Added performance changes
* Changed FAN help string
* Changed HDMI CEC help string
* Changed SATA porting
* Changed SD CARD porting to ready to boot
* Changed UCM porting
* Changed USB port help string
* Changed USB2PP1 porting
* Fixed PCI-E M.2 VDID show error
* Fixed only show two temperature monitor
* Fixed when change BCLK setting cannot flash
* Removed IGD setup item in code
* Removed USCI item
* Removed optane items in setup
* Removed secondary temp sensor options and set to same as primary sensor
* Updated EC FW to 0D.04.00
* Updated ME FW to 11.8.50.3425v2
* Updated RAID OPROM 15.9.0.1015.

**Known Errata:**

* None.

### HNKBLi70.86A.0019.2017. 1219.1818 Development BIOS

**About This Release:**

* Date: December 19, 2017
* ROM Image Checksum: ee0e
* ME Firmware: 11.8.50.3420
* EC Firmware: 0C.04.00
* Memory Reference Code: Based on 2.9.3
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed USB device plugin USB port CON4801 no present OS detect sound
* Fixed USB Port 06[Charging Port] no set to gray out and disable when Portable Device Charging Mode set to Charging Only.
* Fixed WMI pulsing/LAN index value
* Changed VccSA and VccGT to 24A and 60A
* Enabled secure boot after manufacturing mode locked
* Enabled SPI lock
* Added LED Control tab in Devices page
* Updated RC to 2.9.3
* Updated EC FW to 0C.04.00

**Known Errata:**

* Temporarily removed FwBuffer variable within CISDFlashSMIHandler which causes Visual BIOS F7 auto reset.

### HNKBLi70.86A.0018.2017.1206.2304 Development BIOS

**About This Release:**

* Date: December 06, 2017
* ROM Image Checksum: e422
* ME Firmware: 11.8.50.3420
* EC Firmware: 0C.03.00
* Memory Reference Code: Based on 2.9.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added BIOS self recovery setup item
* Added fanless mode
* Added second fan
* Changed LED brightness to 26 steps
* Changed LED default to SW control
* Changed SATA setup items
* Changed TDC
* Changed front led number
* Changed power limit default settings
* Changed psys max to 2960
* Changed video setup items
* Fixed SATA mode change from RAID to AHCI hangs
* Fixed button LED reset to default after reboot
* Fixed fast boot not disable USB KB for setup menu
* Fixed o2micro sd card power saving mode setting
* Fixed power button menu fails while overclocking support default enable
* Updated EC FW to 0C.03.00.

**Known Errata:**

* None.

### HNKBLi70.86A.0017.2017.1130.1224 Development BIOS

**About This Release:**

* Date: November 30, 2017
* ROM Image Checksum: 1f74
* ME Firmware: 11.8.50.3420
* EC Firmware: 0C.02.00
* Memory Reference Code: Based on 2.9.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Removed HDMI/DisplayPort Audio setup item
* Removed Startup Sound setup item
* Removed LED Ready mode items
* Added manual memory timing override function
* Enabled IntelSST
* Fixed tRRD\_L, tRRD\_S value range
* Fixed TBT boot related help string
* Fixed memory voltage/timing/tWR/tRTP help string
* Fixed power button menu function
* Updated EC FW to 0C.02.00

**Known Errata:**

* 0C.XX.XX version EC is for fab C board, HDD LED and LAN LED's behavior is oppsite on fab B board.

### HNKBLi70.86A.0016.2017.1122.2347 Development BIOS

**About This Release:**

* Date: November 22, 2017
* ROM Image Checksum: 8bd6
* ME Firmware: 11.8.50.3420
* EC Firmware: 0B.08.00
* Memory Reference Code: Based on 2.9.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Added CEC setup items
* Changed suppress POST alert message default to Enabled
* Fixed LED WMI setting changed after reboot
* Updated HDD security module
* Fixed USB port disable and no detect function
* Fixed some setup item can change when user access level set to view only
* Fixed IDE password help string

**Known Errata:**

* None.

### HNKBLi70.86A.0015.2017.1117.1801 Development BIOS

**About This Release:**

* Date: November 17, 2017
* ROM Image Checksum: 8164
* ME Firmware: 11.8.50.3420
* EC Firmware: 0B.08.00
* Memory Reference Code: Based on 2.9.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed USB charging setup item
* Fixed USB S4/S5 power setup item
* Fixed fast boot can set when HDD user password installed
* Fixed WMI LED set indicator type issue
* Removed IGD minimum memory option and set to 64MB
* Enabled IntelSST function
* Enabled FPRR feature
* BCLK for F10 load default issue
* Changed IA TDC power limit to 104A
* Changed IccMAX to 104A
* Downgrade ME FW to 11.8.50.3420.

**Known Errata:**

* None.

### HNKBLi70.86A.0014.2017.1115.1741 Development BIOS

**About This Release:**

* Date: November 15, 2017
* ROM Image Checksum: c5f9
* ME Firmware: 11.8.50.3425
* EC Firmware: 0B.08.00
* Memory Reference Code: Based on 2.9.1
* RC: Based on 2.9.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed BLCK function
* Changed LED WMI function
* Updated EC FW to 08.00
* Updated ME FW to 11.8.50.3425
* Updated RC to 2.9.1

**Known Errata:**

* Power button menu not working.

### HNKBLi70.86A.0013.2017.1101.2334 Development BIOS

**About This Release:**

* Date: November 01, 2017
* ROM Image Checksum: 6f63
* ME Firmware: 11.8.50.3399
* EC Firmware: 0B.07.00
* Memory Reference Code: Based on 2.8.1
* RC: Based on 2.8.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1073
* SATA RAID Option ROM: 15.9.0.1013
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Updated ME FW to 11.8.50.3399
* Updated RAID Driver to 15.9.0.1013
* Updated GOP to 9.0.1073
* Updated EC FW to 0B.07.00
* Fixed secure boot can’t install key.
* Fixed USB charging port not working
* Fixed UCSI yellow bang
* Fixed incorrect setup items
* Fixed show hotkey string when flash update

**Known Errata:**

* None.

### HNKBLi70.86A.0012.2017.1026.1357 Development BIOS

**About This Release:**

* Date: October 25, 2017
* ROM Image Checksum: 4f89
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.06.00
* Memory Reference Code: Based on 2.8.1
* RC: Based on 2.8.1
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Updated EC to 0B.06.00
* Updated RC to 2.8.1
* Fixed advanced help text of fast boot setup item
* Fixed M.2 slot detection string in setup
* Added "Portable Device Charging Mode" setup item
* Added "Wake on WLAN and BT Enable" setup item
* Removed RMT mode setup item
* Removed HDMI CEC setup item
* Set PL1/PL2 to 45W/65W
* Changed verb table for TOSLINK
* Enabled Boot Guard support
* Enabled above 4G decoding support
* Changed L1 setting of O2 Micro card reader
* Added performance items
* Changed GPP H4 to bidirectional

**Known Errata:**

* None.

### HNKBLi70.86A.0011.2017.1018.2024 Development BIOS

**About This Release:**

* Date: October 18, 2017
* ROM Image Checksum: a861
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.05.00
* Memory Reference Code: Based on 2.7.2
* RC: Based on 2.7.3
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed wake on lan S5 not working
* Fixed card reader SSID porting
* Updated EC FW
* Updated SMBIOS module to 15
* Changed SMBIOS Type 3 chassis info SKU number default string
* Changed Asmedia USB to GEN1
* Changed verb table setting

**Known Errata:**

* None.

### HNKBLi70.86A.0010.2017.1012.1055 Development BIOS

**About This Release:**

* Date: October 12, 2017
* ROM Image Checksum: 4fc8
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.04.00
* Memory Reference Code: Based on 2.7.2
* RC: Based on 2.7.3
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed error execute QueryLed WMI method.
* Fixed power button menu keyboard not working
* Changed verb table setting
* Updated EC FW to 0B.04.00

**Known Errata:**

* None.

### HNKBLi70.86A.0009.2017.1006.1218 Development BIOS

**About This Release:**

* Date: October 06, 2017
* ROM Image Checksum: 9cff
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.03.00
* Memory Reference Code: Based on 2.7.2
* RC: Based on 2.7.3
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219, 0.0.17 i211
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Fixed i211,i219 PXE ROM not both show on boot menu
* Changed audio verb table setting

**Known Errata:**

* None.

### HNKBLi70.86A.0008.2017.0927.2330 Development BIOS

**About This Release:**

* Date: September 27, 2017
* ROM Image Checksum: 0x3aac
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.03.00
* Memory Reference Code: Based on 2.7.2
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11 i219
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M22906EA\_0000006A.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Updated RC code to 2.7.3 (RS3 BKC)
* Fixed keyboard cannot use with entry DOS
* Fixed USB device can't boot via by thunderbolt
* Fixed TBT3 device lost when resume from sleep mode
* Fixed CIR isn't appear in Device Manager

**Known Errata:**

* None.

### HNKBLi70.86A.0007.2017.0920.2225 Development BIOS

**About This Release:**

* Date: September 20, 2017
* ROM Image Checksum: 0x26c3
* ME Firmware: 11.7.4.3314
* EC Firmware: 0B.03.00
* Memory Reference Code: Based on 2.7.2
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1069
* SATA RAID Option ROM: 15.9.0.1007
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

M22906EA\_0000006A.mcb

M02906EB\_0000005E.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

M22906EA\_0000006A.mcb

M02906EB\_0000005E.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Update RC to 2.7.2
* Added Psys setting
* Added WMI for new LED function implement
* Added Deep SX support
* Added ASM1142 L1 support

**Known Errata:**

* Cannot use iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0006.2017.0914.1116 Development BIOS

**About This Release:**

* Date: September 14, 2017
* ROM Image Checksum: 0x3a15
* ME Firmware: 11.7.3.3307
* EC Firmware: 0B.02.00
* Memory Reference Code: Based on 2.7.0
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.3027
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: 7.5.11
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000006F\_00000070.PDB

* Additional Microcode Updates included only in .BIO File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000006F\_00000070.PDB

**New Fixes/Features:**

* Update RC to 2.7.0
* Fixed optane cannot detect
* Fixed front panel USB not working with setup menu
* Added delay time for GPU power sequence
* Fixed ME device cannot recognize after EC flash
* Fixed EC flash fail
* Fixed PL1/PL2 setting
* Added porting for card reader
* Added RTD3 support for card reader
* Added IMVP8 issue fix
* Changed verb table

**Known Errata:**

* Cannot use iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0005.2017.0830.2140 Development BIOS

**About This Release:**

* Date: August 30, 2017
* ROM Image Checksum: 0xb053
* ME Firmware: 11.7.0.3290
* EC Firmware: 0A.07.00
* Memory Reference Code: Based on 2.6.0
* MEBx Revision: NA
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.1014
* SATA non-RAID Option ROM: NA
* AHCI Code: Based on AHCI\_14
* LAN Option ROM: PXE 2.1 Build 092
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000005D\_0000005E.PDB

* Additional Microcode Updates included only in .BIO File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000005D\_0000005E.PDB

**New Fixes/Features:**

* Added LED control setup option
* Updated fan curve and fan control with EC
* Fixed COM2 yellow bang after resume from S3
* Added ASMEDIA porting for front USB wakeup
* Updated EC firmware to 0A.07.00
* Changed SIRQ default to continuous mode

**Known Errata:**

* Cannot use iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0004.2017.0817.1143 Development BIOS

**About This Release:**

* Date: August 24, 2017
* ROM Image Checksum: 0x22eb
* ME Firmware: 11.7.0.3290
* EC Firmware: 0A.05.00
* Memory Reference Code: Based on 2.6.0.0
* MEBx Revision: N/A
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.1014
* SATA non-RAID Option ROM: N/A
* AHCI Code: Based on 14
* LAN Option ROM: 2.1 Build 092
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000005D\_0000005E.PDB

* Additional Microcode Updates included only in .BIO File:

N/A

**New Fixes/Features:**

* Added fan curve
* Fixed hang 0x04 when quick unplug DC power with RTC battery
* Added USB CHG port not support wake up from S3 solution

**Known Errata:**

* Cannot use iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0003.2017.0817.1143 Development BIOS

**About This Release:**

* Date: August 17, 2017
* ROM Image Checksum: 0xdcdb
* ME Firmware: 11.7.0.3290
* EC Firmware: 0C.02.00
* Memory Reference Code: Based on 2.6.0.0
* MEBx Revision: N/A
* Integrated Graphics
  + - Option ROM: 9.0.1051
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.1014
* SATA non-RAID Option ROM: N/A
* AHCI Code: Based on 14
* LAN Option ROM: 2.1 Build 092
* Visual BIOS: 2.2.25
* Supported Flash Devices:

WinBond W25Q128JVSIQ 16MB

MACRONIX MX25L12850F 16MB

GigaDevice GD25B127D 16MB

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000066.mcb

M2A906E9\_0000005D\_0000005E.PDB

* Additional Microcode Updates included only in .BIO File:

N/A

**New Fixes/Features:**

* Add CISD feature code module
* Updated CRB code to 2.6.0
* Changed dGPU power sequence and GPIO setting
* Fixed not showing option ROM message on post

**Known Errata:**

* Cannot use iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0002.2017.0809.1839 Development BIOS

**About This Release:**

* Date: August 09, 2017
* ROM Image Checksum: 0xec17
* ME Firmware: 11.7.0.3290
* EC Firmware: N/A
* Memory Reference Code: Based on 2.5.0.0
* MEBx Revision: N/A
* Integrated Graphics
  + - Option ROM: N/A
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.3054
* SATA non-RAID Option ROM: N/A
* AHCI Code: Based on 14
* LAN Option ROM: 2.1 Build 092
* Visual BIOS: N/A
* Supported Flash Devices:

MX25L12873FM2I-10G

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000064.mcb

MC0406E3\_000000BA.mcb

M22906EA\_0000005C.mcb

M2A906E9\_0000005E.mcb

M36506E3\_000000BA.mcb

M2A906E9\_0000005D\_0000005E.PDB

* Additional Microcode Updates included only in .BIO File:

N/A

**New Fixes/Features:**

* Changed dGPU power sequence delay from 150ms to 100ms
* Changed verb table subsystem ID for headset
* Changed DMIC related GPIO setting

**Known Errata:**

* Cannot use F7/iflash, can use “fpt -f HN0001.bin” under UEFI shell.

### HNKBLi70.86A.0001.2017.0802.1553 Development BIOS

**About This Release:**

* Date: August 02, 2017
* ROM Image Checksum: 0x0d9e
* ME Firmware: 11.7.0.3290
* EC Firmware: N/A
* Memory Reference Code: Based on 2.5.0.0
* MEBx Revision: N/A
* Integrated Graphics
  + - Option ROM: N/A
    - UEFI Driver: 9.0.1066
* SATA RAID Option ROM: 15.7.0.3054
* SATA non-RAID Option ROM: N/A
* AHCI Code: Based on 14
* LAN Option ROM: 2.1 Build 092
* Visual BIOS: N/A
* Supported Flash Devices:

MX25L12873FM2I-10G

* Microcode Updates included in .ROM File:

MC0806E9\_00000062.mcb

MC0806EA\_00000064.mcb

MC0406E3\_000000BA.mcb

M22906EA\_0000005C.mcb

M2A906E9\_0000005E.mcb

M36506E3\_000000BA.mcb

M2A906E9\_0000005D\_0000005E.PDB

* Additional Microcode Updates included only in .BIO File:

N/A

**New Fixes/Features:**

* First formal release.

**Known Errata:**

* Cannot use F7/iflash, can use “fpt -f HN0001.bin” under UEFI shell.

LEGAL INFORMATION

**Information in this document is provided in connection with Intel Products and for the purpose of supporting Intel developed server/desktop boards and systems.**

No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. Except as provided in Intel's Terms and Conditions of Sale for such products, Intel assumes no liability whatsoever, and Intel disclaims any express or implied warranty, relating to sale and/or use of Intel products including liability or warranties relating to fitness for a particular purpose, merchantability, or infringement of any patent, copyright or other intellectual property right. Intel Corporation may have patents or pending patent applications, trademarks, copyrights, or other intellectual property rights that relate to the presented subject matter. The furnishing of documents and other materials and information does not provide any license, express or implied, by estoppel or otherwise, to any such patents, trademarks, copyrights, or other intellectual property rights. Intel products are not intended for use in medical, lifesaving, or life sustaining applications. Intel may make changes to specifications and product descriptions at any time, without notice.

Intel is a trademark of Intel Corporation in the US and other countries.

Copyright (c) 2009 Intel Corporation.