; Copyright (c) 2009-2017 Intel Corporation
; **********************************************************************************************
; **********************************************************************************************
; **    Filename:  iaStorB.inf
; **    Revision:  DRIVER_INFO
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver
; **               Installs: RSTe AHCI RAID Controller Miniport + RST Filter Driver
; **********************************************************************************************
[Version]
Signature="$Windows NT$"
Provider=%INTEL%
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
CatalogFile=iaStorB.cat
DriverVer=04/20/2017,5.1.0.1098
;
[PackageInfo]
Name=AHCIB
;
[SourceDisksNames]
1 = %DiskId1%,,,""
[DestinationDirs]
DefaultDestDir = 12
;
[ControlFlags]
ExcludeFromSelect = *
;
[Manufacturer]
%INTEL% = INTEL, NTamd64.6.1
;
[iaStorB_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStorB.sys
LoadOrderGroup = SCSI miniport
AddReg         = pnpsafe_pci_addreg
;
[iaStorB_EventLog_Inst]
AddReg = iaStorB_EventLog_AddReg
;
[iaStorB_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorB.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7
;
[iaStorF_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStorF.sys
;
[iaStorF_EventLog_Inst]
AddReg = iaStorF_EventLog_AddReg
;
[iaStorF_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7
;
;********************************************************
;*
;* 64-BIT X86 ARCHITECTURE
;*
;* This section specifies the 64-bit architecture specific INF file entries
;* required to install a driver as a 64-bit compatible driver.
;*
;******************************************************************************
[SourceDisksFiles.amd64]
iaStorB.sys = 1,,,
iaStorF.sys = 1,,,
;
[INTEL.NTamd64.6.1]
;Windows_7_x64 and later
%PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_2827&CC_0104
;
[iaStorB_inst.NTamd64]
CopyFiles=@iaStorB.sys
CopyFiles=@iaStorF.sys
;
[iaStorB_inst.NTamd64.HW]
AddReg = iaStorF_addreg
AddReg = msi_addreg
AddReg = storport_addreg
AddReg = sgpio_addreg
;
[iaStorB_inst.NTamd64.Services]
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst
;
[iaStorF_addreg]
; Layer the RST Filter driver under all Disk class devices as a lower disk class filter
;
HKLM, System\CurrentControlSet\Control\Class\{4d36e967-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF
;
[pnpsafe_pci_addreg]
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x00000008
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8)
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001
;
[DefaultInstall]
OptionDesc = %ServiceDescription%
CopyINF = iaStorB.inf
;
[DefaultInstall.Services]
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst
;
[Strings]
; Localizable Strings
;
diskId1 = "RSTe Installation Disk"
;server
PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc = "Intel(R) C600+/C220+ series chipset sSATA RAID Controller"
;
INTEL = "Intel Corporation"
ServiceDescription = "Intel(R) C600+/C220+ series chipset sSATA RAID Controller Driver"
;
; Non-Localizable Strings
;
SPSVCINST_ASSOCSERVICE = 0x00000002
REG_MULTI_SZ           = 0x00010000
REG_EXPAND_SZ          = 0x00020000
REG_TYPE_DWORD         = 0x00010001
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
;
; MSI enables.
;
[msi_addreg]
HKR, Interrupt Management, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1
;
[storport_addreg]
;;; Enables/Disables Idle Power Management for StorPort
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000001
;;; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255)
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF
;
[sgpio_addreg]
;;; Enable/disable SGPIO support
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LED_Supported, %REG_TYPE_DWORD%, 0x00000001
;
