# Copyright (c) 2009-2017 Intel Corporation
# *****************************************************************************************************
# *****************************************************************************************************
# **    Filename:  txtsetup.oem
# **    Revision:  DRIVER_INFO
# **    Abstract:  Windows* OEM File for Intel(R)Rapid Storage Technology Enterprise RAIDPort VMD Drivers
# *****************************************************************************************************
#
[Disks]
#
# This section lists all disks in the disk set.
#
# <description> is a descriptive name for a disk, used when
#   prompting for the disk
# <tagfile> is a file whose presence allows setup to recognize
#   that the disk is inserted.
# <directory> is where the files are located on the disk.
#
#
disk1 = "Intel(R) Rapid Storage Technology Enterprise Driver" \
#
#
[Defaults]
#
# This section lists the default selection for each 'required'
# hardware component.  If a line is not present for a component,
# the default defaults to the first item in the [<component_name>]
# section (see below).
#
# <component_name> is one of computer, display, keyboard, mouse, scsi
# <id> is a unique <within the component> string to be associated
#   with an option.
#
SCSI = iaVROC_P3500
#
[scsi]
#
# This section lists the options available for a particular component.
#
# <id> is the unique string for the option
# <description> is a text string, presented to the user in a menu
# <key_name> gives the name of the key to be created for the component in
#   HKEY_LOCAL_MACHINE\ControlSet001\Services
#
; iaVROC.inf
iaVROC_P3500 = "Intel() RSTe Volume Management Device(VMD)"
#
[Files.scsi.iaVROC_P3500.NTamd64]
driver = disk1, iaVROC.sys, iaVROC
inf    = disk1, iaVROC.inf
catalog = disk1, iavroc.cat
#
# [HardwareIds.scsi.id]
# <id> corresponds to an id entry in the HwComponent section.
# <deviceId> specifies the device id for a mass storage device.
# <service>  specifies the service to be installed for the device.
# The service is specified by the file name of its executable image without a .sys extension.
#
[HardwareIds.scsi.iaVROC_P3500]
id = "PCI\VEN_8086&DEV_201D", "iaVROC"
#
# [Config.subkey_name]
# Specifies the name of a key under the Services\DriverKey tree where Windows places the specified value.
# <value_name> specifies the name of the value to be set.
# <value_type> specifies the type of the registry entry.
# The value_type can be one of the following: REG_DWORD, REG_BINARY, REG_MULTI_SZ
# <value> specifies the value; its format depends on value_type.
#
[Config.iaVROC]
value = Interrupt Management, 0x00000010
value = Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
value = Interrupt Management\MessageSignaledInterruptProperties, MSISupported, REG_DWORD, 1
value = Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, REG_DWORD, 64
value = Interrupt Management\Affinity Policy, 0x00000010
value = Interrupt Management\Affinity Policy, DevicePolicy, REG_DWORD, 5
#