************************************************************
** ENG *****************************************************
************************************************************
*                                                           
*  Intel(R) Chipset Software Installation Utility
*  Installation Readme
*                                                           
*  NOTE:  This document refers to systems 
*         containing the following Intel chipsets: 
*              Intel(R) 810  Chipset 
*              Intel(R) 810E Chipset
*              Intel(R) 815  Chipset
*              Intel(R) 815E Chipset
*              Intel(R) 815EM Chipset
*              Intel(R) 820 Chipset
*              Intel(R) 820E Chipset
*              Intel(R) 840 Chipset
*              Intel(R) 430TX PCIset 
*              Intel(R) 440BX AGPset 
*              Intel(R) 440DX AGPset 
*              Intel(R) 440EX AGPset 
*              Intel(R) 440GX AGPset 
*              Intel(R) 440LX AGPset 
*              Intel(R) 440MX Chipset 
*              Intel(R) 440ZX AGPset
*              Intel(R) 850 Chipset
*              Intel(R) Celeron(TM) Processor Chipset
*               
*
************************************************************
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Installing the Software
    3A. Installing the Software in Interactive Mode
    3B. Installing the Software in Silent Mode
    3C. List of Available Command Line Flag Options
4.  Verifying Installation of the Software
5.  Contents of the Distribution Package
6.  Identifying the Software Version Number
7.  Troubleshooting

************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) Chipset Software Installation Utility 
installs to the target system the Windows* INF files, 
which outline to the operating system how the 
chipset components will be configured.  This is 
needed for the proper functioning of the following 
features:
   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager

************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
1.  The software included with this distribution 
    package is  designed to operate with the 
    following chipset configurations:

         Intel(R) 810  Chipset 
         Intel(R) 810E Chipset
         Intel(R) 815  Chipset
         Intel(R) 815E Chipset
         Intel(R) 815EM Chipset
         Intel(R) 820  Chipset
         Intel(R) 820E Chipset
         Intel(R) 840 Chipset
         Intel(R) 430TX PCIset 
         Intel(R) 440BX AGPset 
         Intel(R) 440DX AGPset 
         Intel(R) 440EX AGPset 
         Intel(R) 440GX AGPset 
         Intel(R) 440LX AGPset 
         Intel(R) 440MX Chipset 
         Intel(R) 440ZX AGPset                 
         Intel(R) 850 Chipset
         Intel(R) Celeron(TM) Processor Chipset
         
      
2.  One of the following operating systems ("OS") 
    must be installed on the system:
    Windows 95      4.00.950   (Original release)
    Windows 95      4.00.950a  (OSR1)
    Windows 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows 98      4.10.1998  (Original release)
    Windows 98 Second Edition
                    4.10.2222  (Original release)         
    Windows ME      4.90.3000  (Original release)
    Windows 2000    5.00.2195  (Original release)

To verify which operating system has been 
installed on the target system, follow the steps 
below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
    f.  Verify which OS has been installed by reading
        the System information.
                              
3.  The software should be installed on systems 
    with at least 32 MB of system memory.

4.  There should be sufficient hard disc space in 
    the <TEMP> directory (typically 
    C:\WINDOWS\TEMP) of the system on
    which this software is installed.

Please check with your system provider to 
determine which operating system and Intel 
chipset are used in your system.  
************************************************************
* 3.  INSTALLING THE SOFTWARE 
************************************************************
This software may be installed in two modes: 
Interactive or Silent.  The Interactive Mode 
requires user input during installation; the Silent 
Mode does not.

In addition, this software offers a set of command 
line flag options which enable extended 
installation functionality. The command line flags 
are not case-sensitive.  See Section 3C for detailed 
descriptions of these flags.

Important Note:
The Intel(R) Chipset Software Installation Utility is 
distributed in two formats -- self extracting .EXE 
files (INFINST_xxx.EXE) or compressed .ZIP files 
(INFINST_xxx.ZIP).  
Depending on which distribution format is being 
executed, the command-line syntax may differ.  
See Section 3C for more details.

************************************************************
* 3A.  INSTALLING THE SOFTWARE IN 
*         INTERACTIVE MODE
************************************************************
1.  Check the System Requirements.  The 
    operating system must be fully installed and 
    running on the system before running this 
    software.

2.  Close any running applications.  Otherwise, you 
    may experience difficulties.

3.  Run the InstallShield* installation program:
       Self-extracting .EXE distribution: 
      INFINST_AUTOL.EXE
       Compressed .ZIP distribution     : 
      SETUP.EXE

4.  You will be prompted to agree to the licence 
    agreement.  If you do not agree, the Installer 
    will exit before extracting any files.
    
5.  Follow the on-screen instructions and use the 
    default settings to complete the set-up, once 
    the operating system has rebooted.

6.  This completes the installation of the Intel(R) 
    Chipset Software Installation Utility.  

************************************************************
* 3B.  INSTALLING THE SOFTWARE IN SILENT 
*         MODE
************************************************************
1.  Check the System Requirements.  The 
    operating system must be fully installed and 
    running on the system before running this 
    software.

2.  Close any running applications.  Otherwise, you 
    may experience difficulties.

3.  Run the InstallShield installation program:
    For silent install with auto-reboot:
       Self-extracting .EXE distribution: 
      INFINST_AUTOL.EXE -a -b -s
       Compressed .ZIP distribution     : 
      SETUP.EXE -b -s
    - OR -
    For silent install without auto-reboot:
       Self-extracting .EXE distribution: 
      INFINST_AUTOL.EXE -a -s
       Compressed .ZIP distribution     : 
      SETUP.EXE -s

4.  The utility will perform the necessary updates 
    and record the installation status in the 
    following system registry key:
        HKEY_LOCAL_MACHINE\Software\Intel
         \INFInst

5.  If the utility was invoked with the "-b" flag, the 
    system will automatically reboot if the update 
    was successful.

    NOTE:  The system MUST be rebooted for all 
           device updates to take effect.

6.  To determine whether the install was 
    successful, verify the 'install' value in the registry 
    key specified during installation in Step 5.

    The following table describes the various 
    parameter values:

    Value      Type      Data            Description
    ---------  -------   --------        ------------------
   "install"  String    "success"     The installation was 
                                      successful.
                        "fail"        The installation was 
                                      not successful.
                                      No INF files were 
                                      copied to the system.                

  "reboot"  String       "Yes"        A reboot is required 
                                      to complete 
                                      the installation.
                         "No"         No reboot is 
                                      required to complete 
                                      the installation.
                                
  "version"  String  <varies>         Current version 
                                      number of the 
                                      Intel(R) Chipset 
                                      Software 
                                      Installation Utility
                                         
************************************************************
* 3C.  LIST OF AVAILABLE COMMAND LINE 
*          FLAG OPTIONS
************************************************************
The Intel(R) Chipset Software Installation Utility 
supports several command line flags for various 
installation options. 
All command line flags and parameters must be 
separated by a space, except for the language 
code after the '-L' flag.
Due to the different distribution formats available 
for the Intel(R) Chipset Software Installation Utility, 
the command line flag syntax may vary:

1. Self-Extracting .EXE Distribution:
      When installing this software using the .EXE 
     distribution, an extra '-A' must be appended to 
     the INFINST_AUTOL.EXE program call (i.e. 
     INFINST_AUTOL.EXE -A) in order to 
     successfully pass command line parameters.  
     The extra '-A' flag for the self-extracting .EXE 
      package is DIFFERENT from the '-A' 
      command line flag option described below.  

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
          
               INFINST_AUTOL.EXE -A -A (optional -P)

2. Compressed .ZIP Distribution:
      When installing this software using the .ZIP 
      distribution,  there is no need to append any 
      extra flags to the SETUP.EXE program call in 
      order to pass command line flags.

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
                        
               SETUP.EXE -A (optional -P)

Below is a list of all the available command line 
flags that may be used with the program call.  
Note that the '-L' and the '-S' flags MUST be 
specified at the end of the command line 
flag list.

Flag            Description
-------            ------------------
-?              Help flag.  Displays the list of available 
                command line flags.  This parameter 
                works in the Interactive mode only.  

-A             Extracts INF files, README.TXT, 
                and instructions for 
                OEM preload (PRELOAD.TXT) to either 
                "C:\Program Files\Intel\InfInst" or the 
                <Installation Path> directory specified 
                using the '-P' flag.  The software will 
                NOT install these INF files to the system.  
                This flag can be combined only with the 
                '-P' flag option.  
                All other options will be ignored if the '-A' 
                flag is specified. 
                This parameter works in either Silent 
                mode or Interactive mode.

-B              Automatically reboots the system after 
                installation.  
                This flag is ignored if '-A' flag is specified.  
                This parameter works in either Silent 
                mode or Interactive mode.

-L<LangCode>    Forces the InstallShield user 
                interface to display the specified 
                language during set-up.  
                Note that there should be NO spaces 
                between '-L' and the 4-digit language 
                code (see below).  This flag and the '-S' 
                flag must be placed at the end of the 
                command line flag list.  This parameter 
                works in Interactive mode only.

-P <Installation Path>   
                Specifies the HDD location to which the 
               INF program files are copied.  If this flag 
               is not specified at the command line, the 
               <Installation Path> directory is by default 
               assumed to be:
                
                   C:\Program Files\Intel\INFInst
                
                If this flag is used without the
                '-A' option, only README.TXT
               will be copied to 
               <Installation Path>.  The directory name 
               can include spaces.  In this case, 
               however, a pair of double quotes (") 
               must enclose the directory name.  This 
               parameter works in either Silent mode or 
               Interactive mode.

-S              Runs the Installer in silent mode.  No 
                user interface is displayed.   This flag 
                and the '-L' flag must be placed at the 
                end of the command line flag list.
              
Below are the language codes used with the '-L' 
flag:

    Language                   <LangCode>
    -----------------        -------------------
    Chinese (PRC)                 0804
    Chinese (Taiwan)              0404
    Danish                        0006
    Dutch                         0013
    English (UK - International)  0809
    English (US)                  0409
    Finnish                       000B
    French (Canadian)             0C0C
    French (Standard)             040C
    German                        0007
    Italian                       0010
    Japanese                      0011
    Korean                        0012
    Norwegian                     0014
    Polish                        0015
    Portuguese (Brazilian)        0416
    Portuguese (Standard)         0816
    Russian                       0019
    Spanish                       000A
    Swedish                       001D
    Thai                          001E

************************************************************
* 4.  VERIFYING INSTALLATION OF THE 
*       SOFTWARE
************************************************************
Run Device Manager to verify the correct 
installation and usage of the INF files.

For Windows 95, Windows 98 and Windows 98 
Second Edition, Windows ME:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Device Manager tab.
   6.  Click on View Devices by Connection button.
   7.  Click on Plug and Play BIOS, or 
       Advanced Configuration and Power Interface 
       (ACPI) BIOS.
   8.  Click on PCI bus.

For Windows 2000:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Hardware tab.
   6.  Click on Device Manager button.
   7.  From the View menu, select menu item 
       Devices by connection.
   8.  Click on Standard PC, or
       Advanced Configuration and Power Interface 
       (ACPI) PC.
   9.  Click on PCI bus.

After the Device Manager is launched as 
described above, check the descriptions for the 
following entries:

    *** NOTE:  Device Manager will display only the 
               names of devices currently detected in 
               the system.

    Intel(R) 810 Chipset:
        Intel(R) 82810 System and Graphics 
        Controller 
        -or-
        Intel(R) 82810 DC-100 System and Graphics 
        Controller
  
    Intel(R) 810E Chipset:
        Intel(R) 82810E DC-133 System and 
        Graphics Controller 

    Intel(R) 820 Chipset, Intel(R) 820E Chipset:
        Intel(R) 82820 Processor to I/O Controller
        Intel(R) 82820 Processor to AGP Controller

    Intel(R) 840 Chipset:
        Intel(R) 82840 Processor to I/O Controller 
        Intel(R) 82840 Processor to AGP Controller 
        Intel(R) 82840 PCI Bridge 
              
     Intel(R) 82806AA PCI 64-bit Hub:
        Intel(R) 82806AA Advanced Programmable 
         Interrupt Controller
        Intel(R) 82806AA PCI Bridge
        Intel(R) 82806AA Controller (reserved)

    Intel(R) 82801AA I/O Controller Hub (ICH):
        Intel(R) 82801AA LPC Interface Controller 
        Intel(R) 82801AA Ultra ATA Controller 
        Intel(R) 82801AA USB Universal Host 
         Controller 
        Intel(R) 82801AA SMBus Controller 
        Intel(R) 82801AA PCI Bridge 
      
    Intel(R) 82801AB I/O Controller Hub (ICH0):
        Intel(R) 82801AB LPC Interface Controller 
        Intel(R) 82801AB Ultra ATA Controller 
        Intel(R) 82801AB USB Universal Host 
         Controller 
        Intel(R) 82801AB SMBus Controller 
        Intel(R) 82801AB PCI Bridge 

    Intel(R) 82371AB PCI to ISA/IDE Xcelerator 
         (PIIX4):
        Intel(R) 82371AB PCI to ISA bridge 
         (EIO mode)
        Intel(R) 82371AB PCI to ISA bridge 
         (ISA mode)
        Intel(R) 82371AB Power Management 
         Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master 
         IDE Controller
        Intel(R) 82371AB/EB/MB PCI to USB 
         Universal Host Controller
   
    Intel(R) 82371EB/MB PCI to ISA/IDE 
         Xcelerator (PIIX4):
        Intel(R) 82371EB/MB PCI to ISA bridge 
         (EIO mode)
        Intel(R) 82371EB/MB PCI to ISA bridge 
         (ISA mode)
        Intel(R) 82371EB/MB Power Management 
         Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master 
         IDE Controller
        Intel(R) 82371AB/EB/MB PCI to USB 
         Universal Host Controller

    Intel(R) 82371SB PCI to ISA/IDE Xcelerator 
         (PIIX3):
        Intel(R) 82371SB PCI to ISA bridge
        Intel(R) 82371SB PCI Bus Master IDE 
         Controller
        Intel(R) 82371SB PCI to USB Universal Host 
         Controller    

    Intel(R) 440MX Chipset:
        Intel(R) 82440MX Processor to I/O Controller
        Intel(R) 82440MX PCI to ISA Bridge
        Intel(R) 82440MX Power Management 
         Controller
        Intel(R) 82440MX Bus Master IDE Controller
        Intel(R) 82440MX USB Universal Host 
         Controller

    Intel(R) 430TX PCIset:
        Intel(R) 82443TX Processor to PCI bridge

    Intel(R) 440BX AGPset, Intel(R) 440DX AGPset,
        Intel(R) 440ZX AGPset:
        Intel(R) 82443BX/ZX/DX Processor to PCI 
         bridge
        Intel(R) 82443BX/ZX/DX Processor to AGP 
          controller

    Intel(R) 440GX AGPset:
        Intel(R) 82443GX Processor to PCI bridge
        Intel(R) 82443GX Processor to AGP controller

    Intel(R) 440LX AGPset:
        Intel(R) 82443LX Processor to PCI bridge
        Intel(R) 82443LX Processor to AGP controller

    Intel(R) 815 Chipset, Intel(R) 815E Chipset, Intel(R) 
    815EM Chipset:
        Intel(R) 82815 Processor to I/O Controller 
         - 1130 
        Intel(R) 82815 Processor to AGP Controller 
         - 1131 

    Intel(R) 82801BA I/O Controller Hub:
        Intel(R) 82801BA LPC Interface Controller 
         - 2440         
        Intel(R) 82801BA PCI Bridge - 244E   
        Intel(R) 82801BA Ultra ATA Storage 
         Controller - 244B         
        Intel(R) 82801BA/BAM SMBus Controller - 
          2443 
        Intel(R) 82801BA/BAM USB Universal Host 
         Controller - 2442 
        Intel(R) 82801BA/BAM USB Universal Host 
          Controller - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio 
          Controller - 2445

   Intel(R) 82801BAM I/O Controller Hub:        
        Intel(R) 82801BAM LPC Interface Controller 
         - 244C         
        Intel(R) 82801BAM PCI Bridge - 2448       
        Intel(R) 82801BAM Ultra ATA Storage 
         Controller - 244A 
        Intel(R) 82801BA/BAM SMBus Controller - 
          2443 
        Intel(R) 82801BA/BAM USB Universal Host 
         Controller - 2442 
        Intel(R) 82801BA/BAM USB Universal Host 
          Controller - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio 
          Controller - 2445 
 

    Intel(R) 850 Chipset:
        Intel(R) 82850 Processor to I/O Controller - 2530
        Intel(R) 82850 Processor to AGP Controller - 2532

    Intel(R) Celeron(TM) Processor Chipset:
        Intel(R) Celeron(TM) Processor to I/O 
        Controller - 1A10
        Intel(R) Celeron(TM) Processor to I/O 
        Controller - 1A11


10. On certain systems, the following device may 
       also be updated:

     a. Click on View Devices by Connection button.
     b. Click on Plug & Play BIOS, or
         Advanced Configuration and Power Interface 
         (ACPI) BIOS.     
     c. Verify that the following entry is present:
        Intel(R) 82802 Firmware Hub Device -OR-
        Intel(R) Security Driver

************************************************************
* 5.  CONTENTS OF THE DISTRIBUTION 
*       PACKAGE
************************************************************
The Intel(R) Chipset Software Installation Utility 
package contains the following items:

    File(s)       
    -------
    INFINST_AUTOL.EXE -or- 
    INFINST_AUTOL.ZIP
    README.TXT

The version of the software included in the 
distribution package is specified in the file 
RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

After installation on a Windows 95, Windows 98, WIndows ME or 
Windows 2000 system, one or more of the following INF files
are copied to the <Windows>\INF directory:

    File(s)
    -------
    440MXCOR.INF
    440MXIDE.INF
    440MXUSB.INF
    810.INF
    810B.INF
    820.INF
    820B.INF
    840.INF
    850.INF
    ICH2AUD.INF
    ICH2CORE.INF
    ICH2IDE.INF
    ICH2SMB.INF
    ICH2USB.INF
    ICHx.INF
    ICHxIDE.INF
    ICHxSMB.INF
    ICHxUSB.INF
    IFWH.INF
    IHOST.INF
    P64H.INF
    P64HRES.INF
    PIIXXIDE.INF
    PIIXXUSB.INF
    PIIX4.INF
    815.INF
    ICH2CORM.INF
    ICH2IDEM.INF
    CPHOSTA.INF


   *** NOTE:  Only the files that reference the 
              currently detected devices are copied to 
              the system.
              If the -A option is exercised, the files are
              not copied to the <Windows>\INF 
              directory.
              See Section 3C for more information.

One or more of the following digital signature files 
are installed to the <Windows>\CATROOT 
directory on a Windows 98, Windows ME or Windows 2000 system 
ONLY:

    File(s)
    -------
    440MXCOR.CAT
    440MXIDE.CAT
    440MXUSB.CAT
    810.CAT
    820.CAT
    820B.CAT
    840.CAT
    850.CAT
    ICHx.CAT
    ICHxIDE.CAT
    ICHxSMB.CAT
    ICHxUSB.CAT
    IFWH.CAT
    P64H.CAT
    P64HRES.CAT
    815.CAT
    ICH2AUD.CAT
    ICH2CORE.CAT
    ICH2IDE.CAT
    ICH2USB.CAT
    ICH2SMB.CAT
    CPHOSTA.CAT
    ICH2CORM.CAT
    ICH2IDEM.CAT
    CPHOSTA.CAT


   *** NOTE:  Only the files that reference the 
              currently detected devices are copied to 
              the system.
              If the -A option is exercised, the files are
              not copied to the <Windows>\CATROOT 
              directory.
              See Section 3C for more information.              

************************************************************
* 6.  IDENTIFYING THE SOFTWARE VERSION 
*       NUMBER
************************************************************
The version of the software included in the 
distribution package is specified in the file 
RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

The version of the software included in the 
distribution package can also be identified by 
examining the following registry location:

    Key name:   
\\HKEY_LOCAL_MACHINE\Software\Intel\InfInst
    Value name: version

************************************************************
* 7.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements in 
Section 2 above have been satisfied.

Issue:      System locks up during Device Manager 
            Remove or during restart.

Solution:   System lockup can occur during Restart 
            as a result of several possible system 
            issues.  In the event of system lockup, 
            restart the machine and view Device 
            Manager.  If devices are listed properly 
            and the system experiences no further 
            problems, then the .INF file restore process 
            was successful.  If devices are not 
            configured correctly, try re-running the 
            procedures outlined in Section 3.

            If this does not fix problems or further 
            problems are experienced, reinstall the 
            operating system.


Issue:      After running the set-up program and 
            rebooting the machine, Windows reports 
            that it cannot find one of the following files:
                  ESDI_506.pdr

Solution:   Click Browse in the dialogue box where 
            this problem occurs, locate the
 
                 <Windows>\System\IOSubsys

            directory and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new 
            devices.

Issue:      After running the set-up program and 
            rebooting the machine, Windows reports 
            that it cannot find one of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialogue box where 
            this problem occurs, locate the
          
                 <Windows>\System32\drivers 
            (for Windows 98, Windows ME)
                   -or-
                  <Windows>\System           
            (for Windows 95)

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new 
            devices.

Issue:      During set-up, installation stops and 
            prompts for one of the following files:
      
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Ensure that the Windows 95 USB 
            Supplement has been installed prior to 
            running the Intel(R) Chipset Software 
            Installation Utility set-up program.

Issue:      After running the set-up program and 
            rebooting the machine, Windows reports 
            that it cannot find the following file:
                  isapnp.vxd

Solution:   Click Browse in the dialogue box where 
            this problem occurs, locate the

                  <Windows>\System

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new 
            devices.

Issue:      After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was 
            not created or the data of the value 
            "install" is not "success".

Solution:   This is caused by one of the following 
             scenarios:
               - The current system does not contain 
                 a supported operating system, or
               - The current system does not contain 
                 a supported chipset.

            Verify the System Requirements in 
           Section 2.

************************************************************
************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENCE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in 
connection with Intel products.  No licence, 
express or implied, by estoppel or otherwise, to 
any intellectual property rights is granted by this 
document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, 
including liability or warranties relating to fitness for 
a particular purpose, merchantability or 
infringement of any patent, copyright or other 
intellectual property right.  Intel products are not 
intended for use in medical, life-saving, or 
life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and 
liabilities for the use of this document and the 
information contained herein, and assumes no 
responsibility for any errors which may appear in 
this document, nor does Intel make a commitment 
to update the information contained herein.  Intel 
reserves the right to make changes to this 
document at any time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of 
their respective owners.

Copyright (c) Intel Corporation, 1997-2000

